/*
 * Copyright (c) 2013 ETH Zurich. All rights reserved.
 *
 * This file is distributed under the terms in the attached LICENSE file.
 * If you do not find this file, copies can be found by writing to:
 * ETH Zurich D-INFK, CAB F.78, Universitaetstrasse 6, CH-8092 Zurich,
 * Attn: Systems Group.
 */

/*
 * omap44xx_iss_csi2_a_regs2.dev
 *
 * DESCRIPTION: 
 *
 * NOTE: This file has been automatically generated based on the
 * XML files extracted from the TI RDT v1.0.0.4p Tool.
 * Download from here: http://www.ti.com/product/omap4460
 * This means that the file might not be optimal in terms of naming
 * conventions for constants and registers (duplicated
 * namespaces in register and device name etc.).
 * Also, because of the underlying structure from the original XML
 * it's possible that some constants appear multiple times (if they
 * have slightly different descriptions for example).
 *
 * You want to clean that up before using the files for the first time!
 */
 
device omap44xx_iss_csi2_a_regs2 msbfirst ( addr base ) "" {
    
    
    register csi2_ctx_transcodeh_i_0 addr(base, 0x0) "Transcode configuration register: defines horizontal frame cropping" {
        _ 3 mbz;
        hcount 13 rw "Pixels to output per line when the values is between 1 and 8191. Pixels HSKIP-WIDTH pixels are output when HCOUNT=0. WIDTH corresponds to the image width provided by the sensor.";
        _ 3 mbz;
        hskip 13 rw "Pixel to skip horizontally. Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodeh_i_1 addr(base, 0x8) "Transcode configuration register: defines horizontal frame cropping" {
        _ 3 mbz;
        hcount 13 rw "Pixels to output per line when the values is between 1 and 8191. Pixels HSKIP-WIDTH pixels are output when HCOUNT=0. WIDTH corresponds to the image width provided by the sensor.";
        _ 3 mbz;
        hskip 13 rw "Pixel to skip horizontally. Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodeh_i_2 addr(base, 0x10) "Transcode configuration register: defines horizontal frame cropping" {
        _ 3 mbz;
        hcount 13 rw "Pixels to output per line when the values is between 1 and 8191. Pixels HSKIP-WIDTH pixels are output when HCOUNT=0. WIDTH corresponds to the image width provided by the sensor.";
        _ 3 mbz;
        hskip 13 rw "Pixel to skip horizontally. Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodeh_i_3 addr(base, 0x18) "Transcode configuration register: defines horizontal frame cropping" {
        _ 3 mbz;
        hcount 13 rw "Pixels to output per line when the values is between 1 and 8191. Pixels HSKIP-WIDTH pixels are output when HCOUNT=0. WIDTH corresponds to the image width provided by the sensor.";
        _ 3 mbz;
        hskip 13 rw "Pixel to skip horizontally. Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodeh_i_4 addr(base, 0x20) "Transcode configuration register: defines horizontal frame cropping" {
        _ 3 mbz;
        hcount 13 rw "Pixels to output per line when the values is between 1 and 8191. Pixels HSKIP-WIDTH pixels are output when HCOUNT=0. WIDTH corresponds to the image width provided by the sensor.";
        _ 3 mbz;
        hskip 13 rw "Pixel to skip horizontally. Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodeh_i_5 addr(base, 0x28) "Transcode configuration register: defines horizontal frame cropping" {
        _ 3 mbz;
        hcount 13 rw "Pixels to output per line when the values is between 1 and 8191. Pixels HSKIP-WIDTH pixels are output when HCOUNT=0. WIDTH corresponds to the image width provided by the sensor.";
        _ 3 mbz;
        hskip 13 rw "Pixel to skip horizontally. Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodeh_i_6 addr(base, 0x30) "Transcode configuration register: defines horizontal frame cropping" {
        _ 3 mbz;
        hcount 13 rw "Pixels to output per line when the values is between 1 and 8191. Pixels HSKIP-WIDTH pixels are output when HCOUNT=0. WIDTH corresponds to the image width provided by the sensor.";
        _ 3 mbz;
        hskip 13 rw "Pixel to skip horizontally. Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodeh_i_7 addr(base, 0x38) "Transcode configuration register: defines horizontal frame cropping" {
        _ 3 mbz;
        hcount 13 rw "Pixels to output per line when the values is between 1 and 8191. Pixels HSKIP-WIDTH pixels are output when HCOUNT=0. WIDTH corresponds to the image width provided by the sensor.";
        _ 3 mbz;
        hskip 13 rw "Pixel to skip horizontally. Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodev_i_0 addr(base, 0x4) "Transcode configuration register: defines vertical frame cropping" {
        _ 3 mbz;
        vcount 13 rw "Lines to output per frame when the values is between 1 and 8191. Pixels VSKIP-HEIGHT pixels are output when VCOUNT=0. HEIGHT corresponds to the image height provided by the sensor.";
        _ 3 mbz;
        vskip 13 rw "Pixel to skip vertically Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodev_i_1 addr(base, 0xC) "Transcode configuration register: defines vertical frame cropping" {
        _ 3 mbz;
        vcount 13 rw "Lines to output per frame when the values is between 1 and 8191. Pixels VSKIP-HEIGHT pixels are output when VCOUNT=0. HEIGHT corresponds to the image height provided by the sensor.";
        _ 3 mbz;
        vskip 13 rw "Pixel to skip vertically Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodev_i_2 addr(base, 0x14) "Transcode configuration register: defines vertical frame cropping" {
        _ 3 mbz;
        vcount 13 rw "Lines to output per frame when the values is between 1 and 8191. Pixels VSKIP-HEIGHT pixels are output when VCOUNT=0. HEIGHT corresponds to the image height provided by the sensor.";
        _ 3 mbz;
        vskip 13 rw "Pixel to skip vertically Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodev_i_3 addr(base, 0x1C) "Transcode configuration register: defines vertical frame cropping" {
        _ 3 mbz;
        vcount 13 rw "Lines to output per frame when the values is between 1 and 8191. Pixels VSKIP-HEIGHT pixels are output when VCOUNT=0. HEIGHT corresponds to the image height provided by the sensor.";
        _ 3 mbz;
        vskip 13 rw "Pixel to skip vertically Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodev_i_4 addr(base, 0x24) "Transcode configuration register: defines vertical frame cropping" {
        _ 3 mbz;
        vcount 13 rw "Lines to output per frame when the values is between 1 and 8191. Pixels VSKIP-HEIGHT pixels are output when VCOUNT=0. HEIGHT corresponds to the image height provided by the sensor.";
        _ 3 mbz;
        vskip 13 rw "Pixel to skip vertically Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodev_i_5 addr(base, 0x2C) "Transcode configuration register: defines vertical frame cropping" {
        _ 3 mbz;
        vcount 13 rw "Lines to output per frame when the values is between 1 and 8191. Pixels VSKIP-HEIGHT pixels are output when VCOUNT=0. HEIGHT corresponds to the image height provided by the sensor.";
        _ 3 mbz;
        vskip 13 rw "Pixel to skip vertically Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodev_i_6 addr(base, 0x34) "Transcode configuration register: defines vertical frame cropping" {
        _ 3 mbz;
        vcount 13 rw "Lines to output per frame when the values is between 1 and 8191. Pixels VSKIP-HEIGHT pixels are output when VCOUNT=0. HEIGHT corresponds to the image height provided by the sensor.";
        _ 3 mbz;
        vskip 13 rw "Pixel to skip vertically Valid values: 0-8191";
    };
    
    register csi2_ctx_transcodev_i_7 addr(base, 0x3C) "Transcode configuration register: defines vertical frame cropping" {
        _ 3 mbz;
        vcount 13 rw "Lines to output per frame when the values is between 1 and 8191. Pixels VSKIP-HEIGHT pixels are output when VCOUNT=0. HEIGHT corresponds to the image height provided by the sensor.";
        _ 3 mbz;
        vskip 13 rw "Pixel to skip vertically Valid values: 0-8191";
    };
};