/*
 * Copyright (c) 2007, 2008, ETH Zurich. All rights reserved.
 *
 * This file is distributed under the terms in the attached LICENSE file.
 * If you do not find this file, copies can be found by writing to:
 * ETH Zurich D-INFK, Universitaetstrasse 6, CH-8092 Zurich. Attn: Systems Group.
 */

/*
 * lpc_bridge.dev
 *
 * DESCRIPTION: this maps to the PCI configuration space of the LPC bridge
 *              and maps currently only the RCBA register, so that we can
 *              access the base of the chipset configuration which we need
 *              to implement the HPET timer
 * 
 */


device lpc_bridge msbfirst ( pci base ) "LPC bridge PCI config space" {
  register rcba rw pci( base, 0xf0 ) "RCBA" {
    baseaddr    18 "Base Address";
    _           13;
    enable       1 "Enable";
  };
};
