/*
 * Copyright (c) 2016, ETH Zurich. All rights reserved.
 *
 * This file is distributed under the terms in the attached LICENSE file.
 * If you do not find this file, copies can be found by writing to:
 * ETH Zurich D-INFK, Universitaetstrasse 6, CH-8092 Zurich. Attn: Systems Group.
 */

/*
 * msix_e1000.dev
 * According to Intel 82574 gigabit ethernet card
 */
device msix_e1000 lsbfirst ( addr base ) "E1000 MSIx Table Structure" {
  regarray msg_addr addr(base, 0x0)[4;0x10] "Address" type(uint64);
  regarray msg_data addr(base, 0x8)[4;0x10] "Message" type(uint32);
  regarray vec_control addr(base, 0xC)[4;0x10] "Vector Control" type(uint32);
};
